**L20 DOORS/SHUTTERS/HATCHES**
490 AUTOMATIC DOORS:

Manufacturer:

ASSA ABLOY Entrance Systems Limited, Unit 9 Windmill Business Village, Sunbury-on-Thames, Middlesex, TW16 7DY. Tel: 0333 006 3443. Email: architect.uk.aaes@assaabloy.com Web: [www.assaabloyentrance.co.uk](http://www.assaabloyentrance.co.uk)

Models:
Besam SEMI TRANSPARENT TELESCOPIC Sliding Door System, with four sliding door leaves, complete with SL500 operator providing automated operation of the sliding door leaves. Providing full retraction of the doors to maximize the clear open width.

Dimensions:

Frame Height (FH): XXXXmm

Frame Width (FW): XXXXmm

Between Jambs size (COW): to suit FW measurement.

Clear Opening Height (COH): To suit FH measurement.

 (By others: - Prepared opening).

Standard equipment:
System: WALL MOUNTED

Frame finish: SAA or Besam powdercoat finish RAL ref: To be confirmed

Glass type: 10mm laminated or TOUGHENED.

SL500 Operator including normal installation to comply with BS7036/EN16005.
Operation Mode Selector: FLUSH or SURFACE.

Emergency unit: EEU (electrical)

Electric Locking Required: FAIL SAFE / FAIL SECURE / BI-STABLE or NONE

Integrated Air Curtain: YES or NO

Activation and control system:

An Electronic control unit with plug-in connections and power supply.
SC-31M Combined direction and threshold presence detection entry activator.
SC-31M Combined direction and threshold presence detection exit activator.

Safety device(s):

Electronic monitored emergency opening unit.

Automatic reversing.

Monitored two way threshold presence safety system.

Side Screen Safety: MONITORED PRESENCE DETECTION

Locking mechanism:

Mechanical lock: YES or NO, positioned in bottom rail of the door.

Euro Cylinder: SINGLE or DOUBLE

Maintenance:

Warranty with bi-annual service visits for optimum performance and longevity

1 YEAR / 2 YEAR / 3 YEAR / 4 YEAR / 5 YEAR / 10 YEAR

Please consult ASSA ABLOY Entrance Systems Limited technical literature for further details and the quotation for project specific notes.