**L20 DOORS/SHUTTERS/HATCHES**
490 AUTOMATIC DOORS:

Manufacturer:

ASSA ABLOY Entrance Systems Limited, Unit 9 Windmill Business Village, Sunbury-on-Thames, Middlesex, TW16 7DY. Tel: 01932 765 888. Sales fax: 01932 765888. General fax: 01932 765864. Email: rps.uk.besam@assaabloy.com Web: [www.assaabloyentrance.co.uk](http://www.assaabloyentrance.co.uk) or [www.besam.co.uk](http://www.besam.co.uk)

Models:
Besam ADS HERMETIC Sliding Door System, with one sliding door leaf, complete with operator providing automated operation of the sliding door leaf.

Dimensions:

Frame Width (FW): XXXXmm

Frame Height: XXXXmm

(By others: - Prepared opening).

Standard equipment:
System: WALL MOUNTED

Frame finish: SAA or Besam powdercoat finish RAL ref: To be confirmed

Operator including normal installation to comply with BS7036/EN16005.
Operation Mode Selector: FLUSH or SURFACE.

Emergency unit: EEU (electrical)

Electric Locking Required: FAIL SAFE / FAIL SECURE / BI-STABLE or NONE

Activation and control system:

An Electronic control unit with plug-in connections and power supply.
SC-31M Combined direction and threshold presence detection entry activator.
SC-31M Combined direction and threshold presence detection exit activator.

Safety device(s):

Electronic monitored emergency opening unit.

Automatic reversing.

Monitored two way threshold presence safety system.

Side Screen Safety: MONITORED PRESENCE DETECTION

Locking mechanism:

Mechanical Hook lock: ONE or TWO, positioned in meeting door stiles.

Euro Cylinder: SINGLE or DOUBLE

Please consult ASSA ABLOY Entrance Systems Limited technical literature for further details and the quotation for project specific notes.